Building configuration...

Current configuration : 25326 bytes
!
! Last configuration change at 10:36:22 AEST Mon Jan 21 2008 by cisco
! NVRAM config last updated at 10:17:48 AEST Mon Jan 21 2008 by cisco
!
version 12.4
parser config cache interface
parser config interface
no service pad
service timestamps debug datetime msec
service timestamps log datetime msec
no service password-encryption
service internal
service compress-config
service sequence-numbers
!
hostname cellardoor
!
boot-start-marker
boot-end-marker
!
logging buffered 4096
enable secret 5 *************
!
aaa new-model
!
!
aaa authentication login default local
aaa authorization exec default local 
!
!
aaa session-id common
clock timezone AEST 10
clock summer-time GMT recurring
!
!
!
dot11 ssid uc520-data
   vlan 1
   authentication open 
   authentication key-management wpa
   wpa-psk ascii 0 ************
!
dot11 ssid uc520-voice
   vlan 100
   authentication open 
   authentication key-management wpa
   wpa-psk ascii 0 *************
!
ip cef
!
!
ip dhcp relay information trust-all
ip dhcp use vrf connected
ip dhcp excluded-address 10.1.1.1 10.1.1.10
ip dhcp excluded-address 192.168.10.1 192.168.10.10
!
ip dhcp pool phone
   network 10.1.1.0 255.255.255.0
   default-router 10.1.1.1 
   option 150 ip 10.1.1.1 
!
ip dhcp pool data
   import all
   network 192.168.10.0 255.255.255.0
   default-router 192.168.10.1 
   dns-server 172.16.1.50 192.231.203.132 192.231.203.3 
!
!         
ip name-server 172.16.1.50
ip name-server 192.231.203.132
ip name-server 192.231.203.3
ip inspect name SDM_LOW cuseeme
ip inspect name SDM_LOW dns
ip inspect name SDM_LOW ftp
ip inspect name SDM_LOW h323
ip inspect name SDM_LOW https
ip inspect name SDM_LOW icmp
ip inspect name SDM_LOW imap
ip inspect name SDM_LOW pop3
ip inspect name SDM_LOW netshow
ip inspect name SDM_LOW rcmd
ip inspect name SDM_LOW realaudio
ip inspect name SDM_LOW rtsp
ip inspect name SDM_LOW esmtp
ip inspect name SDM_LOW sqlnet
ip inspect name SDM_LOW streamworks
ip inspect name SDM_LOW tftp
ip inspect name SDM_LOW tcp
ip inspect name SDM_LOW udp
ip inspect name SDM_LOW vdolive
!
!
stcapp ccm-group 1
stcapp
!
stcapp feature access-code
!
multilink bundle-name authenticated
!
!
voice call send-alert
voice rtp send-recv
!
voice service voip 
 allow-connections h323 to h323
 allow-connections h323 to sip
 allow-connections sip to h323
 allow-connections sip to sip
 no supplementary-service sip moved-temporarily
 no supplementary-service sip refer
 h323
 sip
  no update-callerid
!
!
voice class codec 1
 codec preference 1 g711ulaw
 codec preference 2 g729r8
!
!
!
!
!
!
!
!
!
!
!
voice translation-rule 1
 rule 1 /0391234567/ /201/
!
voice translation-rule 2
 rule 1 /^0/ //
!
!
voice translation-profile CallBlocking
 translate called 2222
!
voice translation-profile SIPIncoming
 translate called 1
!
voice translation-profile SIPOutgoing
 translate redirect-target 2
!
!
voice-card 0
 no dspfarm
!
!
!
username ABCDE privilege 15 secret 5 ***********
archive
 log config
  logging enable
  logging size 600
  hidekeys
!
!
bridge irb
!
!
!
interface Loopback0
 description $FW_INSIDE$
 ip address 10.1.10.2 255.255.255.252
 ip access-group 101 in
 ip nat inside
 ip virtual-reassembly
!
interface FastEthernet0/0
 description $ETH-WAN$
 no ip address
 ip nat outside
 ip virtual-reassembly
 duplex auto
 speed auto
 pppoe enable group global
 pppoe-client dial-pool-number 1
!
interface Integrated-Service-Engine0/0
 ip unnumbered Loopback0
 ip nat inside
 ip virtual-reassembly
 service-module ip address 10.1.10.1 255.255.255.252
 service-module ip default-gateway 10.1.10.2
!
interface FastEthernet0/1/0
 switchport voice vlan 100
 macro description cisco-phone
!
interface FastEthernet0/1/1
 switchport access vlan 2
 macro description cisco-desktop
 spanning-tree portfast
!
interface FastEthernet0/1/2
 switchport voice vlan 100
 macro description cisco-phone
!
interface FastEthernet0/1/3
 switchport voice vlan 100
 macro description cisco-phone
!
interface FastEthernet0/1/4
 switchport voice vlan 100
 macro description cisco-phone
!
interface FastEthernet0/1/5
 switchport voice vlan 100
 macro description cisco-phone
!
interface FastEthernet0/1/6
 switchport voice vlan 100
 macro description cisco-phone
!
interface FastEthernet0/1/7
 switchport voice vlan 100
 macro description cisco-phone
!
interface FastEthernet0/1/8
 switchport mode trunk
 macro description cisco-switch
!
interface Dot11Radio0/5/0
 no ip address
 !
 encryption vlan 1 mode ciphers aes-ccm 
 !
 encryption vlan 100 mode ciphers aes-ccm 
 !
 ssid uc520-data
 !
 ssid uc520-voice
 !
 speed basic-1.0 basic-2.0 basic-5.5 6.0 9.0 basic-11.0 12.0 18.0 24.0 36.0 48.0 54.0
 station-role root
!
interface Dot11Radio0/5/0.1
 encapsulation dot1Q 1 native
 bridge-group 1
 bridge-group 1 subscriber-loop-control
 bridge-group 1 spanning-disabled
 bridge-group 1 block-unknown-source
 no bridge-group 1 source-learning
 no bridge-group 1 unicast-flooding
!
interface Dot11Radio0/5/0.100
 encapsulation dot1Q 100
 bridge-group 100
 bridge-group 100 subscriber-loop-control
 bridge-group 100 spanning-disabled
 bridge-group 100 block-unknown-source
 no bridge-group 100 source-learning
 no bridge-group 100 unicast-flooding
!
interface Vlan1
 no ip address
 bridge-group 1
 bridge-group 1 spanning-disabled
!
interface Vlan2
 no ip address
 bridge-group 2
!
interface Vlan100
 no ip address
 bridge-group 100
 bridge-group 100 spanning-disabled
!
interface Dialer0
 description $FW_OUTSIDE$
 ip address negotiated
 ip access-group 105 in
 ip mtu 1452
 ip nat outside
 ip inspect SDM_LOW out
 ip virtual-reassembly
 encapsulation ppp
 dialer pool 1
 dialer-group 1
 ppp authentication chap pap callin
 ppp chap hostname ********@internode.on.net
 ppp chap password 0 ********
 ppp pap sent-username *********@internode.on.net password 0 *********
!
interface BVI1
 description $FW_INSIDE$
 ip address 192.168.10.1 255.255.255.0
 ip access-group 102 in
 ip nat inside
 ip virtual-reassembly
 ip tcp adjust-mss 1412
!
interface BVI2
 description $FW_INSIDE$
 ip address 172.16.1.254 255.255.255.0
 ip access-group 104 in
 ip nat inside
 ip virtual-reassembly
!
interface BVI100
 description $FW_INSIDE$
 ip address 10.1.1.1 255.255.255.0
 ip access-group 103 in
 ip nat inside
 ip virtual-reassembly
 ip tcp adjust-mss 1412
!
ip route 0.0.0.0 0.0.0.0 Dialer0
ip route 10.1.10.1 255.255.255.255 Integrated-Service-Engine0/0
!
ip http server
ip http authentication local
ip http secure-server
ip http path flash:
ip nat inside source list 1 interface Dialer0 overload
ip nat inside source static tcp 172.16.1.50 80 interface Dialer0 80
ip nat inside source static tcp 172.16.1.50 443 interface Dialer0 443
ip nat inside source static tcp 172.16.1.50 25 interface Dialer0 25
ip nat inside source static tcp 172.16.1.50 22 interface Dialer0 22
ip nat inside source static tcp 172.16.1.50 115 interface Dialer0 115
ip nat inside source static tcp 172.16.1.50 110 interface Dialer0 110
ip nat inside source static tcp 172.16.1.50 143 interface Dialer0 143
ip nat inside source static tcp 172.16.1.50 993 interface Dialer0 993
ip nat inside source static tcp 172.16.1.50 465 interface Dialer0 465
!
access-list 1 remark SDM_ACL Category=2
access-list 1 permit 192.168.10.0 0.0.0.255
access-list 1 permit 10.1.1.0 0.0.0.255
access-list 1 permit 172.16.1.0 0.0.0.255
access-list 1 permit 10.1.10.0 0.0.0.3
access-list 100 remark auto generated by SDM firewall configuration
access-list 100 remark SDM_ACL Category=1
access-list 100 deny   ip 192.168.10.0 0.0.0.255 any
access-list 100 deny   ip host 255.255.255.255 any
access-list 100 deny   ip 127.0.0.0 0.255.255.255 any
access-list 100 permit ip any any
access-list 101 remark auto generated by SDM firewall configuration
access-list 101 remark SDM_ACL Category=1
access-list 101 remark Auto generated by SDM for NTP (123) 203.12.160.2
access-list 101 permit udp host 203.12.160.2 eq ntp host 10.1.10.2 eq ntp
access-list 101 permit tcp 10.1.1.0 0.0.0.255 eq 2000 any
access-list 101 permit udp 10.1.1.0 0.0.0.255 eq 2000 any
access-list 101 deny   ip 172.16.1.0 0.0.0.255 any
access-list 101 deny   ip 10.1.1.0 0.0.0.255 any
access-list 101 deny   ip 192.168.10.0 0.0.0.255 any
access-list 101 deny   ip host 255.255.255.255 any
access-list 101 deny   ip 127.0.0.0 0.255.255.255 any
access-list 101 permit ip any any
access-list 102 remark auto generated by SDM firewall configuration
access-list 102 remark SDM_ACL Category=1
access-list 102 remark Auto generated by SDM for NTP (123) 203.12.160.2
access-list 102 permit udp host 203.12.160.2 eq ntp host 192.168.10.1 eq ntp
access-list 102 deny   ip 10.1.10.0 0.0.0.3 any
access-list 102 deny   ip 172.16.1.0 0.0.0.255 any
access-list 102 deny   ip 10.1.1.0 0.0.0.255 any
access-list 102 deny   ip host 255.255.255.255 any
access-list 102 deny   ip 127.0.0.0 0.255.255.255 any
access-list 102 permit ip any any
access-list 103 remark auto generated by SDM firewall configuration
access-list 103 remark SDM_ACL Category=1
access-list 103 remark Auto generated by SDM for NTP (123) 203.12.160.2
access-list 103 permit udp host 203.12.160.2 eq ntp host 10.1.1.1 eq ntp
access-list 103 permit tcp 10.1.10.0 0.0.0.3 any eq 2000
access-list 103 permit udp 10.1.10.0 0.0.0.3 any eq 2000
access-list 103 deny   ip 10.1.10.0 0.0.0.3 any
access-list 103 deny   ip 172.16.1.0 0.0.0.255 any
access-list 103 deny   ip 192.168.10.0 0.0.0.255 any
access-list 103 deny   ip host 255.255.255.255 any
access-list 103 deny   ip 127.0.0.0 0.255.255.255 any
access-list 103 permit ip any any
access-list 104 remark auto generated by SDM firewall configuration
access-list 104 remark SDM_ACL Category=1
access-list 104 remark Auto generated by SDM for NTP (123) 203.12.160.2
access-list 104 permit udp host 203.12.160.2 eq ntp host 172.16.1.254 eq ntp
access-list 104 deny   ip 10.1.10.0 0.0.0.3 any
access-list 104 deny   ip 10.1.1.0 0.0.0.255 any
access-list 104 deny   ip 192.168.10.0 0.0.0.255 any
access-list 104 deny   ip host 255.255.255.255 any
access-list 104 deny   ip 127.0.0.0 0.255.255.255 any
access-list 104 permit ip any any
access-list 105 remark auto generated by SDM firewall configuration
access-list 105 remark SDM_ACL Category=1
access-list 105 permit tcp any any eq 465
access-list 105 permit tcp any any eq 993
access-list 105 permit tcp any any eq 143
access-list 105 permit tcp any any eq pop3
access-list 105 permit tcp any any eq 115
access-list 105 permit tcp any any eq 22
access-list 105 permit tcp any any eq smtp
access-list 105 permit tcp any any eq 443
access-list 105 permit tcp any any eq www
access-list 105 remark Auto generated by SDM for NTP (123) 203.12.160.2
access-list 105 permit udp host 203.12.160.2 eq ntp any eq ntp
access-list 105 permit ip host 203.2.134.1 any
access-list 105 deny   ip 10.1.10.0 0.0.0.3 any
access-list 105 deny   ip 172.16.1.0 0.0.0.255 any
access-list 105 deny   ip 10.1.1.0 0.0.0.255 any
access-list 105 deny   ip 192.168.10.0 0.0.0.255 any
access-list 105 permit icmp any any echo-reply
access-list 105 permit icmp any any time-exceeded
access-list 105 permit icmp any any unreachable
access-list 105 deny   ip 10.0.0.0 0.255.255.255 any
access-list 105 deny   ip 172.16.0.0 0.15.255.255 any
access-list 105 deny   ip 192.168.0.0 0.0.255.255 any
access-list 105 deny   ip 127.0.0.0 0.255.255.255 any
access-list 105 deny   ip host 255.255.255.255 any
access-list 105 deny   ip host 0.0.0.0 any
access-list 105 deny   ip any any log
dialer-list 1 protocol ip permit
!
!
!
!
tftp-server APPS-1.0.3.SBN
tftp-server apps11.8-2-2TR2.sbn
tftp-server apps31.8-2-2TR2.sbn
tftp-server apps41.8-2-2TR2.sbn
tftp-server apps70.8-2-2TR2.sbn
tftp-server cmterm_7936.3-3-13-0.bin
tftp-server cnu11.8-2-2TR2.sbn
tftp-server cnu31.8-2-2TR2.sbn
tftp-server cnu41.8-2-2TR2.sbn
tftp-server cnu70.8-2-2TR2.sbn
tftp-server CP7902080002SCCP060817A.sbin
tftp-server CP7921G-1.0.3.LOADS
tftp-server cvm11sccp.8-2-2TR2.sbn
tftp-server cvm31sccp.8-2-2TR2.sbn
tftp-server cvm41sccp.8-2-2TR2.sbn
tftp-server cvm70sccp.8-2-2TR2.sbn
tftp-server dsp11.8-2-2TR2.sbn
tftp-server dsp31.8-2-2TR2.sbn
tftp-server dsp41.8-2-2TR2.sbn
tftp-server dsp70.8-2-2TR2.sbn
tftp-server GUI-1.0.3.SBN
tftp-server jar11sccp.8-2-2TR2.sbn
tftp-server jar31sccp.8-2-2TR2.sbn
tftp-server jar41sccp.8-2-2TR2.sbn
tftp-server jar70sccp.8-2-2TR2.sbn
tftp-server P00308000500.bin
tftp-server P00308000500.loads
tftp-server P00308000500.sb2
tftp-server P00308000500.sbn
tftp-server S00105000200.sbn
tftp-server SCCP11.8-2-2SR2S.loads
tftp-server SCCP31.8-2-2SR2S.loads
tftp-server SCCP41.8-2-2SR2S.loads
tftp-server SCCP70.8-2-2SR2S.loads
tftp-server SYS-1.0.3.SBN
tftp-server term06.default.loads
tftp-server term11.default.loads
tftp-server term31.default.loads
tftp-server term41.default.loads
tftp-server term61.default.loads
tftp-server term70.default.loads
tftp-server term71.default.loads
tftp-server TNUX-1.0.3.SBN
tftp-server TNUXR-1.0.3.SBN
tftp-server WLAN-1.0.3.SBN
tftp-server flash:SCCP42.8-3-2S.loads
tftp-server flash:SCCP45.8-3-2S.loads
tftp-server flash:SCCP75.8-3-2S.loads
tftp-server flash:apps42.8-3-1-22.sbn
tftp-server flash:apps45.8-3-1-22.sbn
tftp-server flash:apps75.8-3-1-22.sbn
tftp-server flash:cnu42.8-3-1-22.sbn
tftp-server flash:cnu45.8-3-1-22.sbn
tftp-server flash:cnu75.8-3-1-22.sbn
tftp-server flash:cvm42sccp.8-3-1-22.sbn
tftp-server flash:cvm45sccp.8-3-1-22.sbn
tftp-server flash:cvm75sccp.8-3-1-22.sbn
tftp-server flash:dsp42.8-3-1-22.sbn
tftp-server flash:dsp45.8-3-1-22.sbn
tftp-server flash:dsp75.8-3-1-22.sbn
tftp-server flash:jar42sccp.8-3-1-22.sbn
tftp-server flash:jar45sccp.8-3-1-22.sbn
tftp-server flash:jar75sccp.8-3-1-22.sbn
tftp-server flash:term42.default.loads
tftp-server flash:term45.default.loads
tftp-server flash:term62.default.loads
tftp-server flash:term65.default.loads
tftp-server flash:term75.default.loads
tftp-server DistinctiveRingList.xml
tftp-server RingList.xml
tftp-server flash:AreYouThereF.raw
tftp-server flash:Bass.raw
tftp-server flash:CallBack.raw
tftp-server flash:Chime.raw
tftp-server flash:Classic1.raw
tftp-server flash:Classic2.raw
tftp-server flash:ClockShop.raw
tftp-server flash:Drums1.raw
tftp-server flash:Drums2.raw
tftp-server flash:FilmScore.raw
tftp-server flash:HarpSynth.raw
tftp-server flash:Jamaica.raw
tftp-server flash:KotoEffect.raw
tftp-server flash:MusicBox.raw
tftp-server flash:Piano1.raw
tftp-server flash:Piano2.raw
tftp-server flash:Pop.raw
tftp-server flash:Pulse1.raw
tftp-server flash:Ring1.raw
tftp-server flash:Ring2.raw
tftp-server flash:Ring3.raw
tftp-server flash:Ring4.raw
tftp-server flash:Ring5.raw
tftp-server flash:Ring6.raw
tftp-server flash:Ring7.raw
tftp-server flash:Sax1.raw
tftp-server flash:Sax2.raw
tftp-server flash:Vibe.raw
tftp-server flash:Analog1.raw
tftp-server flash:Analog2.raw
tftp-server flash:AreYouThere.raw
!
control-plane
!
bridge 1 route ip
bridge 2 protocol ieee
bridge 2 route ip
bridge 100 route ip
!
!
voice-port 0/0/0
 timeouts ringing infinity
!
voice-port 0/0/1
 timeouts ringing infinity
!
voice-port 0/0/2
 timeouts ringing infinity
!
voice-port 0/0/3
 timeouts ringing infinity
!
voice-port 0/1/0
 supervisory disconnect dualtone mid-call
 cptone AU
 timeouts ringing infinity
 connection plar 301
 impedance complex1
 caller-id enable
!
voice-port 0/1/1
 connection plar opx 698
 caller-id enable
!
voice-port 0/1/2
 connection plar opx 698
 caller-id enable
!
voice-port 0/1/3
 connection plar opx 698
 caller-id enable
!         
voice-port 0/4/0
 auto-cut-through
 signal immediate
 input gain auto-control -15
 description Music On Hold Port
!
sccp local Loopback0
sccp ccm 10.1.1.1 identifier 1 
sccp
!
sccp ccm group 1
 associate ccm 1 priority 1
!
dial-peer cor custom
 name internal
 name local
 name domestic
 name international
 name 900
 name 976
!
!
dial-peer cor list call-internal
 member internal
!
dial-peer cor list call-local
 member local
!
dial-peer cor list call-domestic
 member domestic
!
dial-peer cor list call-international
 member international
!
dial-peer cor list call-900
 member 900
!
dial-peer cor list call-976
 member 976
!
dial-peer cor list user-internal
 member internal
!
dial-peer cor list user-local
 member internal
 member local
!
dial-peer cor list user-domestic
 member internal
 member local
 member domestic
!
dial-peer cor list user-international
 member internal
 member local
 member domestic
 member international
!
dial-peer cor list user900-internal
 member internal
 member 900
 member 976
!
dial-peer cor list user900-local
 member internal
 member local
 member 900
 member 976
!
dial-peer cor list user900-domestic
 member internal
 member local
 member domestic
 member 900
 member 976
!
dial-peer cor list user900-international
 member internal
 member local
 member domestic
 member international
 member 900
 member 976
!
!
dial-peer voice 1 pots
 service stcapp
 port 0/0/0
!
dial-peer voice 2 pots
 service stcapp
 port 0/0/1
!
dial-peer voice 3 pots
 service stcapp
 port 0/0/2
!
dial-peer voice 4 pots
 service stcapp
 port 0/0/3
!
dial-peer voice 5 pots
 description ** MOH Port **
 destination-pattern ABC
 port 0/4/0
 no sip-register
!
dial-peer voice 50 pots
 description ** FXO pots dial-peer **
 preference 1
 destination-pattern 000
 port 0/1/0
 forward-digits 3
 no sip-register
!
dial-peer voice 2000 voip
 description ** cue voicemail pilot number **
 destination-pattern 699
 session protocol sipv2
 session target ipv4:10.1.10.1
 dtmf-relay sip-notify
 codec g711ulaw
 no vad
!
dial-peer voice 2001 voip
 description ** cue auto attendant number **
 translation-profile outgoing PSTN_CallForwarding
 destination-pattern 698
 session protocol sipv2
 session target ipv4:10.1.10.1
 dtmf-relay sip-notify
 codec g711ulaw
 no vad
!
dial-peer voice 57 pots
 description ** FXO pots dial-peer **
 incoming called-number .
 direct-inward-dial
 port 0/1/0
!
dial-peer voice 2003 voip
 description **Incoming call from SIP trunk**
 translation-profile incoming SIPIncoming
 voice-class codec 1
 voice-class sip dtmf-relay force rtp-nte
 session protocol sipv2
 session target sip-server
 incoming called-number .%
 dtmf-relay rtp-nte
 no vad
!
dial-peer voice 2004 voip
 description **OG to local**
 translation-profile outgoing SIPOutgoing
 destination-pattern 0..........
 voice-class codec 1
 voice-class sip dtmf-relay force rtp-nte
 session protocol sipv2
 session target sip-server
 dtmf-relay rtp-nte
 no vad
!
dial-peer voice 52 pots
 description **Change OG to pots**
 preference 1
 destination-pattern *..........
 port 0/1/0
 forward-digits 10
 no sip-register
!
dial-peer voice 51 pots
 description ** FXO pots dial-peer **
 preference 1
 destination-pattern 0000
 port 0/1/0
 forward-digits 3
 no sip-register
!
!
no dial-peer outbound status-check pots
sip-ua 
 authentication username 0391234567 password 7 *********
 no remote-party-id
 retry invite 2
 retry register 10
 timers connect 100
 mwi-server ipv4:10.1.10.1 expires 86400 port 5060 transport udp 
 registrar dns:sip.internode.on.net expires 240
 sip-server dns:sip.internode.on.net
  host-registrar
!
!
!
telephony-service
 video
 load 7960-7940 P00308000500
 load 7914 S00105000200
 load 7902 CP7902080002SCCP060817A
 load 7921 CP7921G-1.0.3
 load 7931 SCCP31.8-2-2SR2S
 load 7941GE SCCP41.8-2-2SR2S
 load 7941 SCCP41.8-2-2SR2S
 load 7961GE SCCP41.8-2-2SR2S
 load 7961 SCCP41.8-2-2SR2S
 load 7975 SCCP75.8-3-2S
 load 7965 SCCP45.8-3-2S
 load 7945 SCCP45.8-3-2S
 load 7942 SCCP42.8-3-2S
 load 7962 SCCP42.8-3-2S
 load 7971 SCCP70.8-2-2SR2S
 load 7970 SCCP70.8-2-2SR2S
 load 7936 cmterm_7936.3-3-13-0
 load 7906 SCCP11.8-2-2SR2S
 load 7911 SCCP11.8-2-2SR2S
 max-ephones 14
 max-dn 56
 ip source-address 10.1.1.1 port 2000
 auto assign 10 to 19
 auto assign 5 to 8 type anl
 calling-number initiator
 service phone videoCapability 1
 timeouts interdigit 3
 system message Capital IT
 url services http://10.1.10.1/voiceview/common/login.do
 url authentication http://10.1.10.1/voiceview/authentication/authenticate.do
 time-zone 47
 date-format dd-mm-yy
 voicemail 699
 max-conferences 8 gain -6
 call-forward pattern .T
 call-forward system redirecting-expanded
 moh music-on-hold.au
 multicast moh 239.10.16.16 port 2000
 web admin system name cisco secret 5 ************
 dn-webedit 
 time-webedit 
 transfer-system full-consult dss
 transfer-pattern 9.T
 transfer-pattern .T
 secondary-dialtone 0
 create cnf-files version-stamp 7960 Jan 18 2008 12:13:12
!
!
ephone-template  15
 button-layout 7931 2
!
!
ephone-dn  5  dual-line
 number 301 secondary 0394171848 no-reg primary
 label 301
 description Home Phone
 name Home Phone
 call-forward busy 699
 call-forward noan 699 timeout 20
!
!
ephone-dn  6  dual-line
 number 302 no-reg primary
 label 302
 description PhoneB Analog
 name PhoneB Analog
 call-forward busy 699
 call-forward noan 699 timeout 10
 corlist incoming user-domestic
 translation-profile incoming CallBlocking
!
!
ephone-dn  7  dual-line
 number 303 no-reg primary
 label 303
 description PhoneC Analog
 name PhoneC Analog
 call-forward busy 699
 call-forward noan 699 timeout 10
 corlist incoming user-domestic
 translation-profile incoming CallBlocking
!
!
ephone-dn  8  dual-line
 number 304 no-reg primary
 label 304
 description PhoneD Analog
 name PhoneD Analog
 call-forward busy 699
 call-forward noan 699 timeout 10
 corlist incoming user-domestic
 translation-profile incoming CallBlocking
!
!
ephone-dn  9
 number BCD no-reg primary
 description MoH
 moh ip 239.10.16.8 port 2139 out-call ABC
!         
!
ephone-dn  10  dual-line
 number 201 secondary 0391234567 no-reg primary
 label Hello Me
 description Phone
 name Me Phone
 call-forward busy 699
 call-forward noan 699 timeout 20
 mwi sip
!
!
ephone-dn  11  dual-line
 number 202 no-reg primary
 label 202
 description 202
 name 202
 call-forward busy 699
 call-forward noan 699 timeout 10
!
!
ephone-dn  12  dual-line
 number 203 no-reg primary
 label 203
 description 203
 name 203
!
!
ephone-dn  13  dual-line
 number 204 no-reg primary
 label 204
 description 204
 name 204
!
!
ephone-dn  14  dual-line
 number 205 no-reg primary
 label 205
 description 205
 name 205
!
!
ephone-dn  15  dual-line
 number 206 no-reg primary
 label 206
 description 206
 name 206
!
!
ephone-dn  16  dual-line
 number 207 no-reg primary
 label 207
 description 207
 name 207
!
!
ephone-dn  17  dual-line
 number 208 no-reg primary
 label 208
 description 208
 name 208
!
!
ephone-dn  18  dual-line
 number 209 no-reg primary
 label 209
 description 209
 name 209
!
!
ephone-dn  19  dual-line
 number 210 no-reg primary
 label 210
 description 210
 name 210
!
!
ephone-dn  55
 number A801... no-reg primary
 mwi off
!
!
ephone-dn  56
 number A800... no-reg primary
 mwi on
!
!
ephone  1
 device-security-mode none
 mac-address B8FA.D6EC.0000
 username "home"
 type anl
 button  1:5
 pin 1234
!
!
!

!
!
!
line con 0
 no modem enable
line aux 0
line 2
 no activation-character
 no exec
 transport preferred none
 transport input all
line vty 5 100
!         
ntp master
ntp server 203.12.160.2 key 0 prefer

!
webvpn cef
end