Not working!

Xmodem file system is available.
flashfs[0]: 8 files, 3 directories
flashfs[0]: 0 orphaned files, 0 orphaned directories
flashfs[0]: Total bytes: 15998976
flashfs[0]: Bytes used: 4953600
flashfs[0]: Bytes available: 11045376
flashfs[0]: flashfs fsck took 28 seconds.
Base ethernet MAC Address: 00:07:0e:2a:85:0e
Initializing ethernet port 0...
Reset ethernet port 0...
Reset done!
ethernet link up, 100 mbps, full-duplex
Ethernet port 0 initialized: link is up
Loading "flash:/c1130-k9w8-mx.123-11.JA3/c1130-k9w8-mx.123-11.JA3"...###################################################################################################################################################################################################################################################################

File "flash:/c1130-k9w8-mx.123-11.JA3/c1130-k9w8-mx.123-11.JA3" uncompressed and installed, entry point: 0x3000
executing...

              Restricted Rights Legend

Use, duplication, or disclosure by the Government is
subject to restrictions as set forth in subparagraph
(c) of the Commercial Computer Software - Restricted
Rights clause at FAR sec. 52.227-19 and subparagraph
(c) (1) (ii) of the Rights in Technical Data and Computer
Software clause at DFARS sec. 252.227-7013.

           cisco Systems, Inc.
           170 West Tasman Drive
           San Jose, California 95134-1706

Cisco IOS Software, C1130 Software (C1130-K9W8-M), Version 12.3(11)JA3, RELEASE SOFTWARE (fc1)
Technical Support: http://www.cisco.com/techsupport
Copyright (c) 1986-2007 by Cisco Systems, Inc.
Compiled Mon 02-Apr-07 11:28 by pwade
Image text-base: 0x00003000, data-base: 0x00526F00

Initializing flashfs...

flashfs[1]: 8 files, 3 directories
flashfs[1]: 0 orphaned files, 0 orphaned directories
flashfs[1]: Total bytes: 15998976
flashfs[1]: Bytes used: 4953600
flashfs[1]: Bytes available: 11045376
flashfs[1]: flashfs fsck took 4 seconds.
flashfs[1]: Initialization complete....done Initializing flashfs.
cisco AIR-LAP1131AG-E-K9   (PowerPCElvis) processor (revision A0) with 24566K/8192K bytes of memory.
Processor board ID FCZ1131Q09Y
PowerPCElvis CPU at 262Mhz, revision number 0x0950
Last reset from power-on
LWAPP image version 4.0.217.0
1 FastEthernet interface
2 802.11 Radio(s)

32K bytes of flash-simulated non-volatile configuration memory.
Base ethernet MAC Address: 00:07:0E:2A:85:0E
Part Number                          : 73-8962-12
PCA Assembly Number                  : 800-24818-11
PCA Revision Number                  : B0
PCB Serial Number                    : FOC11292SJC
Top Assembly Part Number             : 800-29144-02
Top Assembly Serial Number           : FCZ1131Q09Y
Top Revision Number                  : A0
Product/Model Number                 : AIR-LAP1131AG-E-K9

Press RETURN to get started!

*Mar  1 00:00:05.534: %SOAP_FIPS-2-SELF_TEST_IOS_SUCCESS: IOS crypto FIPS self test passed
*Mar  1 00:00:07.005: %SOAP_FIPS-2-SELF_TEST_RAD_SUCCESS: RADIO crypto FIPS self test passed on interface Dot11Radio 0
*Mar  1 00:00:07.358: %LINK-5-CHANGED: Interface Dot11Radio1, changed state to reset
*Mar  1 00:00:08.555: %SOAP_FIPS-2-SELF_TEST_RAD_SUCCESS: RADIO crypto FIPS self test passed on interface Dot11Radio 1
*Mar  1 00:00:09.660: %SYS-6-LOGGERSTART: Logger process started
*Mar  1 00:00:09.717: %CDP_PD-4-POWER_OK: Full power - AC_ADAPTOR inline power source
*Mar  1 00:00:09.723: %SYS-5-RESTART: System restarted --
Cisco IOS Software, C1130 Software (C1130-K9W8-M), Version 12.3(11)JA3, RELEASE SOFTWARE (fc1)
Technical Support: http://www.cisco.com/techsupport
Copyright (c) 1986-2007 by Cisco Systems, Inc.
Compiled Mon 02-Apr-07 11:28 by pwade
*Mar  1 00:00:09.723: %SNMP-5-COLDSTART: SNMP agent on host AP0007.0e2a.850e is undergoing a cold start
*Mar  1 00:00:09.804: %DOT11-6-FREQ_SCAN: Interface Dot11Radio0, Scanning frequencies for 16 seconds
*Mar  1 00:00:10.594: %LINK-3-UPDOWN: Interface FastEthernet0, changed state to up
*Mar  1 00:00:10.739: %LINEPROTO-5-UPDOWN: Line protocol on Interface Dot11Radio1, changed state to down
*Mar  1 00:00:10.776: %LINEPROTO-5-UPDOWN: Line protocol on Interface Dot11Radio0, changed state to down
*Mar  1 00:00:11.594: %LINEPROTO-5-UPDOWN: Line protocol on Interface FastEthernet0, changed state to up
*Mar  1 00:00:25.812: %DOT11-6-FREQ_USED: Interface Dot11Radio0, frequency 2422 selected
*Mar  1 00:00:25.825: %LINK-3-UPDOWN: Interface Dot11Radio0, changed state to up
*Mar  1 00:00:26.825: %LINEPROTO-5-UPDOWN: Line protocol on Interface Dot11Radio0, changed state to up
*Mar  1 00:00:28.737: %LWAPP-5-CHANGED: LWAPP changed state to DISCOVERY
*Mar  1 00:00:28.762: %LINK-5-CHANGED: Interface Dot11Radio0, changed state to reset
*Mar  1 00:00:28.771: %LINK-3-UPDOWN: Interface Dot11Radio1, changed state to up
*Mar  1 00:00:28.799: %LINK-3-UPDOWN: Interface Dot11Radio0, changed state to up
*Mar  1 00:00:28.801: %LINK-3-UPDOWN: Interface Dot11Radio1, changed state to down
*Mar  1 00:00:28.802: %LINK-5-CHANGED: Interface Dot11Radio1, changed state to reset
*Mar  1 00:00:28.870: %LINK-3-UPDOWN: Interface Dot11Radio1, changed state to up
*Mar  1 00:00:29.870: %LINEPROTO-5-UPDOWN: Line protocol on Interface Dot11Radio1, changed state to up
*Mar  1 00:00:36.876: %DHCP-6-ADDRESS_ASSIGN: Interface FastEthernet0 assigned DHCP address 10.68.131.115, mask 255.255.128.0, hostname AP0007.0e2a.850e

Translating "CISCO-LWAPP-CONTROLLER.customerdomainname.com"...domain server (10.68.128.1) [OK]