|  |  |  |
| --- | --- | --- |
| CE의 하드웨어 교체시 license을 업데이트해야하는 경우 | Platform | : VDS-TC |
| Software | : All |
| Author | : Jung Hyun Su |
| Date | : 2013/12/23 |
| Docu. No | : CKT-VIDEO-00001 |

**1. Problem Description:**

CE의 하드웨어 교체시 license을 업데이트해야 하는 경우에 대해서 알아 보도록 하겠습니다.

**2. Explanation:**

VDS-TC caching engine(CE)에서 하드웨어의 불량으로 chassis, CPU 또는 internal harddisk을 교체할 경우가 있을 수 있으며 필요에 따라서는 license도 업데이트 할 경우가 생길 수 있습니다.

License는 chassis ID/Serial number와 관련이 있으며, chassis을 교체하는 경우에는 반드시 license을 업데이트 해야 합니다.

CPU나 internal harddisk교체 시에는 license을 업데이트가 필요가 없습니다.

자세한 정보는 아래에 있는 troubleshooting 가이드의 1장과 6장을 참조하시길 바랍니다.

[http://www.cisco.com/en/US/docs/video/videoscape/distribution\_suite/vds/v5\_0\_2/OL-29792-01\_VDS\_TC\_5.0.2\_TS\_guide.pdf](http%3A%2F%2Fwww.cisco.com%2Fen%2FUS%2Fdocs%2Fvideo%2Fvideoscape%2Fdistribution_suite%2Fvds%2Fv5_0_2%2FOL-29792-01_VDS_TC_5.0.2_TS_guide.pdf)

**3. Action Plan: n/a**

**4. Reference:**

Troubleshooting 가이드

[http://www.cisco.com/en/US/docs/video/videoscape/distribution\_suite/vds/v5\_0\_2/OL-29792-01\_VDS\_TC\_5.0.2\_TS\_guide.pdf](http%3A%2F%2Fwww.cisco.com%2Fen%2FUS%2Fdocs%2Fvideo%2Fvideoscape%2Fdistribution_suite%2Fvds%2Fv5_0_2%2FOL-29792-01_VDS_TC_5.0.2_TS_guide.pdf)