008327: Sep 14 21:07:06.850: //-1/xxxxxxxxxxxx/SIP/Msg/ccsipDisplayMsg:

Sent:

INVITE sip:14143322701@66.23.129.253:5060 SIP/2.0

Via: SIP/2.0/UDP 98.103.52.140:5060;branch=z9hG4bK48CB1F63

Remote-Party-ID: "301" <sip:301@98.103.52.140>;party=calling;screen=no;privacy=off

From: "301" <sip:301@66.23.129.253>;tag=965502D4-0

To: <sip:14143322701@66.23.129.253>

Date: Tue, 14 Sep 2010 21:07:06 GMT

Call-ID: DD8E78E3-BF7A11DF-B5E5805D-57B3653B@98.103.52.140

Supported: 100rel,timer,resource-priority,replaces,sdp-anat

Min-SE: 1800

Cisco-Guid: 3704621913-3212448223-3051389021-1471374651

User-Agent: Cisco-SIPGateway/IOS-12.x

Allow: INVITE, OPTIONS, BYE, CANCEL, ACK, PRACK, UPDATE, REFER, SUBSCRIBE, NOTIFY, INFO, REGISTER

CSeq: 101 INVITE

Max-Forwards: 70

Timestamp: 1284498426

Contact: <sip:301@98.103.52.140:5060>

Expires: 180

Allow-Events: telephone-event

Content-Type: application/sdp

Content-Disposition: session;handling=required

Content-Length: 250

v=0

o=CiscoSystemsSIP-GW-UserAgent 3184 4916 IN IP4 98.103.52.140

s=SIP Call

c=IN IP4 98.103.52.140

t=0 0

m=audio 17338 RTP/AVP 0 101

c=IN IP4 98.103.52.140

a=rtpmap:0 PCMU/8000

a=rtpmap:101 telephone-event/8000

a=fmtp:101 0-16

a=ptime:20

008328: Sep 14 21:07:06.902: //-1/xxxxxxxxxxxx/SIP/Msg/ccsipDisplayMsg:

Received:

SIP/2.0 407 Proxy Authentication Required

Via: SIP/2.0/UDP 98.103.52.140:5060;branch=z9hG4bK48CB1F63;rport=52425

From: "301" <sip:301@66.23.129.253>;tag=965502D4-0

To: <sip:14143322701@66.23.129.253>;tag=9c6a9fdfd4d16ebaa52f34c4c528cbe5.0229

Call-ID: DD8E78E3-BF7A11DF-B5E5805D-57B3653B@98.103.52.140

CSeq: 101 INVITE

Proxy-Authenticate: Digest realm="nexvortex.com", nonce="4c8fe55e30648743e8f0f6d48b1742ac65d014a0"

Server: Sip EXpress router (0.9.6 (i386/linux))

Content-Length: 0

Warning: 392 192.168.1.50:5060 "Noisy feedback tells: pid=14651 req\_src\_ip=98.103.52.140 req\_src\_port=52425 in\_uri=sip:14143322701@66.23.129.253:5060 out\_uri=sip:14143322701@66.23.129.253:5060 via\_cnt==1"

008329: Sep 14 21:07:06.906: //-1/xxxxxxxxxxxx/SIP/Msg/ccsipDisplayMsg:

Sent:

ACK sip:14143322701@66.23.129.253:5060 SIP/2.0

Via: SIP/2.0/UDP 98.103.52.140:5060;branch=z9hG4bK48CB1F63

From: "301" <sip:301@66.23.129.253>;tag=965502D4-0

To: <sip:14143322701@66.23.129.253>;tag=9c6a9fdfd4d16ebaa52f34c4c528cbe5.0229

Date: Tue, 14 Sep 2010 21:07:06 GMT

Call-ID: DD8E78E3-BF7A11DF-B5E5805D-57B3653B@98.103.52.140

Max-Forwards: 70

CSeq: 101 ACK

Allow-Events: telephone-event

Content-Length: 0

008330: Sep 14 21:07:06.906: //-1/xxxxxxxxxxxx/SIP/Msg/ccsipDisplayMsg:

Sent:

INVITE sip:14143322701@66.23.129.253:5060 SIP/2.0

Via: SIP/2.0/UDP 98.103.52.140:5060;branch=z9hG4bK48CC1367

Remote-Party-ID: "301" <sip:301@98.103.52.140>;party=calling;screen=no;privacy=off

From: "301" <sip:301@66.23.129.253>;tag=965502D4-0

To: <sip:14143322701@66.23.129.253>

Date: Tue, 14 Sep 2010 21:07:06 GMT

Call-ID: DD8E78E3-BF7A11DF-B5E5805D-57B3653B@98.103.52.140

Supported: 100rel,timer,resource-priority,replaces,sdp-anat

Min-SE: 1800

Cisco-Guid: 3704621913-3212448223-3051389021-1471374651

User-Agent: Cisco-SIPGateway/IOS-12.x

Allow: INVITE, OPTIONS, BYE, CANCEL, ACK, PRACK, UPDATE, REFER, SUBSCRIBE, NOTIFY, INFO, REGISTER

CSeq: 102 INVITE

Max-Forwards: 70

Timestamp: 1284498426

Contact: <sip:301@98.103.52.140:5060>

Expires: 180

Allow-Events: telephone-event

Proxy-Authorization: Digest username="sY6330XFBw",realm="nexvortex.com",uri="sip:14143322701@66.23.129.253:5060",response="541a392b6bc8a081cd41aa7f29952e6a",nonce="4c8fe55e30648743e8f0f6d48b1742ac65d014a0",algorithm=md5

Content-Type: application/sdp

Content-Disposition: session;handling=required

Content-Length: 250

v=0

o=CiscoSystemsSIP-GW-UserAgent 3184 4916 IN IP4 98.103.52.140

s=SIP Call

c=IN IP4 98.103.52.140

t=0 0

m=audio 17338 RTP/AVP 0 101

c=IN IP4 98.103.52.140

a=rtpmap:0 PCMU/8000

a=rtpmap:101 telephone-event/8000

a=fmtp:101 0-16

a=ptime:20

008331: Sep 14 21:07:07.026: //-1/xxxxxxxxxxxx/SIP/Msg/ccsipDisplayMsg:

Received:

SIP/2.0 100 trying -- your call is important to us

Via: SIP/2.0/UDP 98.103.52.140:5060;branch=z9hG4bK48CC1367;rport=52425

From: "301" <sip:301@66.23.129.253>;tag=965502D4-0

To: <sip:14143322701@66.23.129.253>

Call-ID: DD8E78E3-BF7A11DF-B5E5805D-57B3653B@98.103.52.140

CSeq: 102 INVITE

Server: Sip EXpress router (0.9.6 (i386/linux))

Content-Length: 0

Warning: 392 192.168.1.50:5060 "Noisy feedback tells: pid=14714 req\_src\_ip=98.103.52.140 req\_src\_port=52425 in\_uri=sip:14143322701@66.23.129.253:5060 out\_uri=sip:14143322701@67.216.35.162:5060 via\_cnt==1"

008332: Sep 14 21:07:09.806: //-1/xxxxxxxxxxxx/SIP/Msg/ccsipDisplayMsg:

Received:

SIP/2.0 180 Ringing

Via: SIP/2.0/UDP 98.103.52.140:5060;rport=52425;branch=z9hG4bK48CC1367

Record-Route: <sip:14143322701@66.23.129.253:5060;nat=yes;ftag=965502D4-0;lr=on>

From: "301" <sip:301@66.23.129.253>;tag=965502D4-0

To: <sip:14143322701@66.23.129.253>;tag=gsscd82075f9df42d83a6f724b03de8926a

Call-ID: DD8E78E3-BF7A11DF-B5E5805D-57B3653B@98.103.52.140

CSeq: 102 INVITE

Server: Gafachi UAS v110.09

Allow: INVITE, ACK, CANCEL, OPTIONS, BYE

Contact: <sip:14143322701@67.216.35.162>

Content-Type: application/sdp

Content-Length: 234

v=0

o=root 594381718 594381718 IN IP4 67.216.38.5

s=session

c=IN IP4 67.216.38.5

t=0 0

m=audio 38356 RTP/AVP 0 101

a=rtpmap:0 PCMU/8000

a=rtpmap:101 telephone-event/8000

a=fmtp:101 0-15

a=silenceSupp:off - - - -

a=ptime:20

008333: Sep 14 21:07:14.742: //-1/xxxxxxxxxxxx/SIP/Msg/ccsipDisplayMsg:

Received:

SIP/2.0 200 OK

Via: SIP/2.0/UDP 98.103.52.140:5060;rport=52425;branch=z9hG4bK48CC1367

Record-Route: <sip:14143322701@66.23.129.253:5060;nat=yes;ftag=965502D4-0;lr=on>

From: "301" <sip:301@66.23.129.253>;tag=965502D4-0

To: <sip:14143322701@66.23.129.253>;tag=gsscd82075f9df42d83a6f724b03de8926a

Call-ID: DD8E78E3-BF7A11DF-B5E5805D-57B3653B@98.103.52.140

CSeq: 102 INVITE

Server: Gafachi UAS v110.09

Allow: INVITE, ACK, CANCEL, OPTIONS, BYE

Contact: <sip:14143322701@67.216.35.162>

Content-Type: application/sdp

Content-Length: 234

v=0

o=root 594381718 594381719 IN IP4 67.216.38.5

s=session

c=IN IP4 67.216.38.5

t=0 0

m=audio 38356 RTP/AVP 0 101

a=rtpmap:0 PCMU/8000

a=rtpmap:101 telephone-event/8000

a=fmtp:101 0-15

a=silenceSupp:off - - - -

a=ptime:20

008334: Sep 14 21:07:14.754: //-1/xxxxxxxxxxxx/SIP/Msg/ccsipDisplayMsg:

Sent:

ACK sip:14143322701@67.216.35.162:5060 SIP/2.0

Via: SIP/2.0/UDP 98.103.52.140:5060;branch=z9hG4bK48CD127F

From: "301" <sip:301@66.23.129.253>;tag=965502D4-0

To: <sip:14143322701@66.23.129.253>;tag=gsscd82075f9df42d83a6f724b03de8926a

Date: Tue, 14 Sep 2010 21:07:06 GMT

Call-ID: DD8E78E3-BF7A11DF-B5E5805D-57B3653B@98.103.52.140

Route: <sip:14143322701@66.23.129.253:5060;nat=yes;ftag=965502D4-0;lr=on>

Max-Forwards: 70

CSeq: 102 ACK

Proxy-Authorization: Digest username="sY6330XFBw",realm="nexvortex.com",uri="sip:14143322701@66.23.129.253:5060",response="541a392b6bc8a081cd41aa7f29952e6a",nonce="4c8fe55e30648743e8f0f6d48b1742ac65d014a0",algorithm=md5

Allow-Events: telephone-event

Content-Length: 0